- Power Messages
  - Configure Information
- Power Summary
  - Power Information
  - Thermal Information
  - Supply Information
- Power Details
  - Power By Block Type
  - Power By Hierarchy
  - Power By Clock Domain

# Power Messages

Report Title | Power Analysis Report
Design File | Z:\hdmi\impl\gwsynthesis\hdmi.vg
Physical Constraints File | Z:\hdmi\src\hdmi.cst
Timing Constraints File | Z:\hdmi\src\hdmi.sdc
Tool Version | V1.9.12 (64-bit)
Part Number | GW1NR-LV9QN88PC6/I5
Device | GW1NR-9
Device Version | C
Created Time | Wed Apr 1 21:06:43 2026
Legal Announcement | Copyright (C)2014-2025 Gowin Semiconductor Corporation. All rights reserved.

## Configure Information:

Grade | Commercial
Process | Typical
Ambient Temperature | 25.000
Use Custom Theta JA | false
Heat Sink | None
Air Flow | LFM_0
Use Custom Theta SA | false
Board Thermal Model | None
Use Custom Theta JB | false
Related Vcd File |
Related Saif File |
Filter Glitches | false
Default IO Toggle Rate | 0.125
Default Remain Toggle Rate | 0.125

# Power Summary

## Power Information:

Total Power (mW) | 47.886
Quiescent Power (mW) | 26.615
Dynamic Power (mW) | 21.272
Psram Power (mW) | 86.000

## Thermal Information:

Junction Temperature | 25.993
Theta JA | 21.450
Max Allowed Ambient Temperature | 84.007

## Supply Information:

Voltage Source | Voltage | Dynamic Current(mA) | Quiescent Current(mA) | Power(mW)
--- | --- | --- | --- | ---
VCC | 1.200 | 15.122 | 3.511 | 22.359
VCCX | 3.300 | 0.485 | 5.000 | 18.102
VCCIO18 | 1.800 | 0.052 | 0.490 | 0.976
VCCIO33 | 3.300 | 0.433 | 1.521 | 6.450

# Power Details

## Power By Block Type:

Block Type | Total Power(mW) | Static Power(mW) | Average Toggle Rate(millions of transitions/sec)
--- | --- | --- | ---
Logic | 0.522 | NA | 4.864
IO | 11.195 | 7.474 | 7.298
BSRAM | 13.502 | NA | NA
PLL | 3.515 | NA | NA

## Power By Hierarchy:

Hierarchy Entity | Total Power(mW) | Block Dynamic Power(mW)
--- | --- | ---
top | 17.539 | 17.539(17.535)
top/ps2_1/ | 0.026 | 0.026(0.000)
top/serial_1/ | 0.020 | 0.020(0.000)
top/spi_1/ | 0.023 | 0.023(0.000)
top/svo_hdmi_inst/ | 13.811 | 13.811(13.811)
top/svo_hdmi_inst/svo_enc/ | 0.022 | 0.022(0.000)
top/svo_hdmi_inst/svo_overlay/ | 0.006 | 0.006(0.006)
top/svo_hdmi_inst/svo_overlay/svo_buf_in/ | 0.003 | 0.003(0.002)
top/svo_hdmi_inst/svo_overlay/svo_buf_in/svo_axis_pipe/ | 0.002 | 0.002(0.000)
top/svo_hdmi_inst/svo_overlay/svo_buf_out/ | 0.003 | 0.003(0.002)
top/svo_hdmi_inst/svo_overlay/svo_buf_out/svo_axis_pipe/ | 0.002 | 0.002(0.000)
top/svo_hdmi_inst/svo_overlay/svo_buf_over/ | 0.001 | 0.001(0.000)
top/svo_hdmi_inst/svo_overlay/svo_buf_over/svo_axis_pipe/ | 0.000 | 0.000(0.000)
top/svo_hdmi_inst/svo_tcard/ | 13.711 | 13.711(13.550)
top/svo_hdmi_inst/svo_tcard/grmode1/ | 0.010 | 0.010(0.000)
top/svo_hdmi_inst/svo_tcard/txtmode0/ | 0.087 | 0.087(0.000)
top/svo_hdmi_inst/svo_tcard/your_instance_name/ | 13.453 | 13.453(0.000)
top/svo_hdmi_inst/svo_term/ | 0.005 | 0.005(0.000)
top/svo_hdmi_inst/svo_tmds_0/ | 0.022 | 0.022(0.000)
top/svo_hdmi_inst/svo_tmds_1/ | 0.022 | 0.022(0.000)
top/svo_hdmi_inst/svo_tmds_2/ | 0.022 | 0.022(0.000)
top/test1/ | 0.133 | 0.133(0.064)
top/test1/dac1/ | 0.006 | 0.006(0.000)
top/test1/env1/ | 0.025 | 0.025(0.000)
top/test1/toneA/ | 0.009 | 0.009(0.000)
top/test1/toneB/ | 0.009 | 0.009(0.000)
top/test1/toneC/ | 0.009 | 0.009(0.000)
top/test1/wng1/ | 0.007 | 0.007(0.001)
top/test1/wng1/lfsr1/ | 0.001 | 0.001(0.000)
top/timer_1/ | 0.005 | 0.005(0.000)
top/u_Reset_Sync/ | 0.002 | 0.002(0.000)
top/u_pll/ | 3.515 | 3.515(0.000)

## Power By Clock Domain:

Clock Domain | Clock Frequency(Mhz) | Total Dynamic Power(mW)
--- | --- | ---
cpuclk | 50.000 | 0.374
NO CLOCK DOMAIN | 0.000 | 0.000
test1/wng1/fsr_clk | 50.000 | 0.003
u_div_5/clkdiv_inst/CLKOUT.default_gen_clk | 25.200 | 4.711
svo_hdmi_inst/svo_tcard/bram_aclock | 50.000 | 8.947
u_pll/rpll_inst/CLKOUT.default_gen_clk | 126.000 | 0.002
clk_osc | 27.000 | 3.515