- PnR Messages
- PnR Details
- Resource
  - Resource Usage Summary
  - I/O Bank Usage Summary
  - Clock Resource Usage Summary
  - Global Clock Signals
  - Pinout by Port Name
  - All Package Pins

# PnR Messages

Report Title | PnR Report
Design File | Z:\hdmi\impl\gwsynthesis\hdmi.vg
Physical Constraints File | Z:\hdmi\src\hdmi.cst
Timing Constraints File | Z:\hdmi\src\hdmi.sdc
Tool Version | V1.9.12 (64-bit)
Part Number | GW1NR-LV9QN88PC6/I5
Device | GW1NR-9
Device Version | C
Created Time | Wed Apr 1 21:06:43 2026
Legal Announcement | Copyright (C)2014-2025 Gowin Semiconductor Corporation. All rights reserved.

# PnR Details

Place & Route Process | Running placement: Placement Phase 0: CPU time = 0h 0m 0.569s, Elapsed time = 0h 0m 0.569s Placement Phase 1: CPU time = 0h 0m 0.054s, Elapsed time = 0h 0m 0.054s Placement Phase 2: CPU time = 0h 0m 0.334s, Elapsed time = 0h 0m 0.334s Placement Phase 3: CPU time = 0h 0m 1s, Elapsed time = 0h 0m 1s Total Placement: CPU time = 0h 0m 2s, Elapsed time = 0h 0m 2s Running routing: Routing Phase 0: CPU time = 0h 0m 0s, Elapsed time = 0h 0m 0.001s Routing Phase 1: CPU time = 0h 0m 0.569s, Elapsed time = 0h 0m 0.569s Routing Phase 2: CPU time = 0h 0m 2s, Elapsed time = 0h 0m 2s Routing Phase 3: CPU time = 0h 0m 0s, Elapsed time = 0h 0m 0s Total Routing: CPU time = 0h 0m 2s, Elapsed time = 0h 0m 2s Generate output files: CPU time = 0h 0m 1s, Elapsed time = 0h 0m 1s
Total Time and Memory Usage | CPU time = 0h 0m 6s, Elapsed time = 0h 0m 6s, Peak memory usage = 360MB

# Resource

## Resource Usage Summary:

Resource | Usage | Utilization
Logic | 2156/8640 | 25%
--LUT,ALU,ROM16 | 2132(1727 LUT, 405 ALU, 0 ROM16) | -
--SSRAM(RAM16) | 4 | -
Register | 1104/6693 | 17%
--Logic Register as Latch | 0/6480 | 0%
--Logic Register as FF | 1092/6480 | 17%
--I/O Register as Latch | 0/213 | 0%
--I/O Register as FF | 12/213 | 6%
CLS | 1477/4320 | 35%
I/O Port | 47/71 | 67%
I/O Buf | 43 | -
--Input Buf | 13 | -
--Output Buf | 20 | -
--Inout Buf | 10 | -
IOLOGIC | 3 OSER10 | 7%
BSRAM | 19 DPB 1 pROM | 77%

## I/O Bank Usage Summary:

I/O Bank | Usage | Utilization
bank 1 | 19/25 | 76%
bank 2 | 17/23 | 74%
bank 3 | 11/23 | 48%

## Clock Resource Usage Summary:

Clock Resource | Usage | Utilization
PRIMARY | 4/8 | 50%
LW | 2/8 | 25%
GCLK_PIN | 3/3 | 100%
CLKDIV | 1/8 | 13%
rPLL | 1/2 | 50%

## Global Clock Signals:

Signal | Global Clock | Location
cpuclk_d | PRIMARY | TR TL BR BL
clk_p | PRIMARY | TR TL BR BL
test1/wng1/fsr_clk | PRIMARY | BL
svo_hdmi_inst/svo_tcard/bram_aclock | PRIMARY | TR TL BR BL
nrst_d | LW | -
svo_hdmi_inst/n147_5 | LW | -
clk_d | HCLK | BANK4_BANK5_HCLK0
clk_p5 | HCLK | BANK0_BANK1_HCLK0

## Pinout by Port Name:

Port Name | Diff Pair | Loc./Bank | Constraint | Dir. | Site | CFG | IO Type | Drive | Pull Mode | PCI Clamp | Hysteresis | Open Drain | Vref | Single Resistor | Diff Resistor | BankVccio
ncs | - | 34/2 | Y | in | IOB23[B] | - | LVCMOS33 | NA | UP | ON | NONE | NA | NA | NA | NA | 3.3
nwr | - | 28/2 | Y | in | IOB11[B] | - | LVCMOS33 | NA | UP | ON | NONE | NA | NA | NA | NA | 3.3
nrd | - | 29/2 | Y | in | IOB13[A] | - | LVCMOS33 | NA | UP | ON | NONE | NA | NA | NA | NA | 3.3
nrst | - | 30/2 | Y | in | IOB13[B] | - | LVCMOS33 | NA | UP | ON | NONE | NA | NA | NA | NA | 3.3
addr[0] | - | 82/3 | Y | in | IOT11[A] | - | LVCMOS18 | NA | UP | ON | NONE | NA | NA | OFF | NA | 1.8
addr[1] | - | 81/3 | Y | in | IOT11[B] | - | LVCMOS18 | NA | UP | ON | NONE | NA | NA | OFF | NA | 1.8
addr[2] | - | 80/3 | Y | in | IOT12[A] | - | LVCMOS18 | NA | UP | ON | NONE | NA | NA | OFF | NA | 1.8
addr[3] | - | 79/3 | Y | in | IOT12[B] | - | LVCMOS18 | NA | UP | ON | NONE | NA | NA | OFF | NA | 1.8
cpuclk | - | 33/2 | Y | in | IOB23[A] | - | LVCMOS33 | NA | UP | ON | NONE | NA | NA | NA | NA | 3.3
rxd_serial | - | 27/2 | Y | in | IOB11[A] | - | LVCMOS33 | NA | UP | ON | NONE | NA | NA | NA | NA | 3.3
disk_miso | - | 39/2 | Y | in | IOB33[A] | - | LVCMOS33 | NA | UP | ON | NONE | NA | NA | NA | NA | 3.3
clk | - | 52/1 | Y | in | IOR17[A] | GCLKT_3 | LVCMOS33 | NA | UP | ON | NONE | NA | NA | OFF | NA | 3.3
resetn | - | 4/3 | Y | in | IOL5[A] | JTAGSEL_N/LPLL_T_in | LVCMOS18 | NA | UP | ON | NONE | NA | NA | OFF | NA | 1.8
intr_out | - | 40/2 | Y | out | IOB33[B] | - | LVCMOS33 | 8 | NONE | NA | NA | OFF | NA | NA | NA | 3.3
led[0] | - | 10/3 | Y | out | IOL15[A] | GCLKT_6 | LVCMOS18 | 8 | UP | NA | NA | OFF | NA | OFF | NA | 1.8
led[1] | - | 11/3 | Y | out | IOL16[B] | - | LVCMOS18 | 8 | UP | NA | NA | OFF | NA | OFF | NA | 1.8
led[2] | - | 13/3 | Y | out | IOL21[B] | - | LVCMOS18 | 8 | UP | NA | NA | OFF | NA | OFF | NA | 1.8
led[3] | - | 14/3 | Y | out | IOL22[B] | - | LVCMOS18 | 8 | UP | NA | NA | OFF | NA | OFF | NA | 1.8
led[4] | - | 15/3 | Y | out | IOL25[B] | - | LVCMOS18 | 8 | UP | NA | NA | OFF | NA | OFF | NA | 1.8
led[5] | - | 16/3 | Y | out | IOL26[B] | - | LVCMOS18 | 8 | UP | NA | NA | OFF | NA | OFF | NA | 1.8
dacser | - | 49/1 | Y | out | IOR24[A] | - | LVCMOS33 | 8 | UP | NA | NA | OFF | NA | OFF | NA | 3.3
dacsclk | - | 31/2 | Y | out | IOB15[A] | - | LVCMOS33 | 8 | UP | NA | NA | OFF | NA | NA | NA | 3.3
dacrclk | - | 32/2 | Y | out | IOB15[B] | - | LVCMOS33 | 8 | UP | NA | NA | OFF | NA | NA | NA | 3.3
txd_serial | - | 26/2 | Y | out | IOB8[B] | - | LVCMOS33 | 8 | UP | NA | NA | OFF | NA | NA | NA | 3.3
rts_serial | - | 63/1 | Y | out | IOR5[A] | RPLL_T_in | LVCMOS33 | 8 | UP | NA | NA | OFF | NA | OFF | NA | 3.3
disk_mosi | - | 37/2 | Y | out | IOB31[A] | - | LVCMOS33 | 8 | UP | NA | NA | OFF | NA | NA | NA | 3.3
disk_sck | - | 36/2 | Y | out | IOB29[B] | GCLKC_4 | LVCMOS33 | 8 | UP | NA | NA | OFF | NA | NA | NA | 3.3
disk_cs | - | 76/1 | Y | out | IOT37[B] | - | LVCMOS33 | 8 | UP | NA | NA | OFF | NA | OFF | NA | 3.3
disk_reset | - | 77/1 | Y | out | IOT37[A] | - | LVCMOS33 | 8 | UP | NA | NA | OFF | NA | OFF | NA | 3.3
tmds_clk_n | tmds_clk_p | 68/1 | Y | out | IOT42[B] | - | LVCMOS33D | 8 | NA | NA | NA | NA | NA | OFF | NA | 3.3
tmds_clk_p | tmds_clk_n | 69/1 | Y | out | IOT42[A] | - | LVCMOS33D | 8 | NONE | NA | NA | NA | NA | OFF | NA | 3.3
tmds_d_n[0] | tmds_d_p[0] | 70/1 | Y | out | IOT41[B] | - | LVCMOS33D | 8 | NA | NA | NA | NA | NA | OFF | NA | 3.3
tmds_d_n[1] | tmds_d_p[1] | 72/1 | Y | out | IOT39[B] | - | LVCMOS33D | 8 | NA | NA | NA | NA | NA | OFF | NA | 3.3
tmds_d_n[2] | tmds_d_p[2] | 74/1 | Y | out | IOT38[B] | - | LVCMOS33D | 8 | NA | NA | NA | NA | NA | OFF | NA | 3.3
tmds_d_p[0] | tmds_d_n[0] | 71/1 | Y | out | IOT41[A] | - | LVCMOS33D | 8 | NONE | NA | NA | NA | NA | OFF | NA | 3.3
tmds_d_p[1] | tmds_d_n[1] | 73/1 | Y | out | IOT39[A] | - | LVCMOS33D | 8 | NONE | NA | NA | NA | NA | OFF | NA | 3.3
tmds_d_p[2] | tmds_d_n[2] | 75/1 | Y | out | IOT38[A] | - | LVCMOS33D | 8 | NONE | NA | NA | NA | NA | OFF | NA | 3.3
data[0] | - | 41/2 | Y | io | IOB41[A] | - | LVCMOS33 | 8 | UP | NA | NONE | OFF | NA | NA | NA | 3.3
data[1] | - | 42/2 | Y | io | IOB41[B] | - | LVCMOS33 | 8 | UP | NA | NONE | OFF | NA | NA | NA | 3.3
data[2] | - | 51/1 | Y | io | IOR17[B] | GCLKC_3 | LVCMOS33 | 8 | UP | NA | NONE | OFF | NA | OFF | NA | 3.3
data[3] | - | 53/1 | Y | io | IOR15[B] | DOUT/WE_N | LVCMOS33 | 8 | UP | NA | NONE | OFF | NA | OFF | NA | 3.3
data[4] | - | 54/1 | Y | io | IOR15[A] | DIN/CLKHOLD_N | LVCMOS33 | 8 | UP | NA | NONE | OFF | NA | OFF | NA | 3.3
data[5] | - | 55/1 | Y | io | IOR14[B] | SSPI_CS_N/D0 | LVCMOS33 | 8 | UP | NA | NONE | OFF | NA | OFF | NA | 3.3
data[6] | - | 56/1 | Y | io | IOR14[A] | SO/D1 | LVCMOS33 | 8 | UP | NA | NONE | OFF | NA | OFF | NA | 3.3
data[7] | - | 57/1 | Y | io | IOR13[A] | FASTRD_N/D3 | LVCMOS33 | 8 | UP | NA | NONE | OFF | NA | OFF | NA | 3.3
ps2data | - | 35/2 | Y | io | IOB29[A] | GCLKT_4 | LVCMOS33 | 8 | NONE | NA | NONE | OFF | NA | NA | NA | 3.3
ps2clk | - | 25/2 | Y | io | IOB8[A] | - | LVCMOS33 | 8 | NONE | NA | NONE | OFF | NA | NA | NA | 3.3

## All Package Pins:

Loc./Bank | Signal | Dir. | Site | CFG | IO Type | Drive | Pull Mode | PCI Clamp | Hysteresis | Open Drain | Vref | Single Resistor | Diff Resistor | Bank Vccio
3/3 | - | in | IOT2[A] | - | LVCMOS18 | NA | UP | ON | NONE | NA | NA | NA | NA | 1.8
88/3 | - | in | IOT5[A] | MODE0 | LVCMOS18 | NA | UP | ON | NONE | NA | NA | NA | NA | 1.8
87/3 | - | in | IOT6[B] | MODE1 | LVCMOS18 | NA | UP | ON | NONE | NA | NA | NA | NA | 1.8
86/3 | - | in | IOT8[A] | - | LVCMOS18 | NA | UP | ON | NONE | NA | NA | NA | NA | 1.8
85/3 | - | in | IOT8[B] | - | LVCMOS18 | NA | UP | ON | NONE | NA | NA | NA | NA | 1.8
84/3 | - | in | IOT10[A] | - | LVCMOS18 | NA | UP | ON | NONE | NA | NA | NA | NA | 1.8
83/3 | - | in | IOT10[B] | - | LVCMOS18 | NA | UP | ON | NONE | NA | NA | NA | NA | 1.8
82/3 | addr[0] | in | IOT11[A] | - | LVCMOS18 | NA | UP | ON | NONE | NA | NA | OFF | NA | 1.8
81/3 | addr[1] | in | IOT11[B] | - | LVCMOS18 | NA | UP | ON | NONE | NA | NA | OFF | NA | 1.8
80/3 | addr[2] | in | IOT12[A] | - | LVCMOS18 | NA | UP | ON | NONE | NA | NA | OFF | NA | 1.8
79/3 | addr[3] | in | IOT12[B] | - | LVCMOS18 | NA | UP | ON | NONE | NA | NA | OFF | NA | 1.8
77/1 | disk_reset | out | IOT37[A] | - | LVCMOS33 | 8 | UP | NA | NA | OFF | NA | OFF | NA | 3.3
76/1 | disk_cs | out | IOT37[B] | - | LVCMOS33 | 8 | UP | NA | NA | OFF | NA | OFF | NA | 3.3
75/1 | tmds_d_p[2] | out | IOT38[A] | - | LVCMOS33D | 8 | NONE | NA | NA | NA | NA | OFF | NA | 3.3
74/1 | tmds_d_n[2] | out | IOT38[B] | - | LVCMOS33D | 8 | NA | NA | NA | NA | NA | OFF | NA | 3.3
73/1 | tmds_d_p[1] | out | IOT39[A] | - | LVCMOS33D | 8 | NONE | NA | NA | NA | NA | OFF | NA | 3.3
72/1 | tmds_d_n[1] | out | IOT39[B] | - | LVCMOS33D | 8 | NA | NA | NA | NA | NA | OFF | NA | 3.3
71/1 | tmds_d_p[0] | out | IOT41[A] | - | LVCMOS33D | 8 | NONE | NA | NA | NA | NA | OFF | NA | 3.3
70/1 | tmds_d_n[0] | out | IOT41[B] | - | LVCMOS33D | 8 | NA | NA | NA | NA | NA | OFF | NA | 3.3
69/1 | tmds_clk_p | out | IOT42[A] | - | LVCMOS33D | 8 | NONE | NA | NA | NA | NA | OFF | NA | 3.3
68/1 | tmds_clk_n | out | IOT42[B] | - | LVCMOS33D | 8 | NA | NA | NA | NA | NA | OFF | NA | 3.3
17/2 | - | in | IOB2[A] | - | LVCMOS33 | NA | UP | ON | NONE | NA | NA | NA | NA | 3.3
18/2 | - | in | IOB2[B] | - | LVCMOS33 | NA | UP | ON | NONE | NA | NA | NA | NA | 3.3
19/2 | - | in | IOB4[A] | - | LVCMOS33 | NA | UP | ON | NONE | NA | NA | NA | NA | 3.3
20/2 | - | in | IOB4[B] | - | LVCMOS33 | NA | UP | ON | NONE | NA | NA | NA | NA | 3.3
25/2 | ps2clk | io | IOB8[A] | - | LVCMOS33 | 8 | NONE | NA | NONE | OFF | NA | NA | NA | 3.3
26/2 | txd_serial | out | IOB8[B] | - | LVCMOS33 | 8 | UP | NA | NA | OFF | NA | NA | NA | 3.3
27/2 | rxd_serial | in | IOB11[A] | - | LVCMOS33 | NA | UP | ON | NONE | NA | NA | NA | NA | 3.3
28/2 | nwr | in | IOB11[B] | - | LVCMOS33 | NA | UP | ON | NONE | NA | NA | NA | NA | 3.3
29/2 | nrd | in | IOB13[A] | - | LVCMOS33 | NA | UP | ON | NONE | NA | NA | NA | NA | 3.3
30/2 | nrst | in | IOB13[B] | - | LVCMOS33 | NA | UP | ON | NONE | NA | NA | NA | NA | 3.3
31/2 | dacsclk | out | IOB15[A] | - | LVCMOS33 | 8 | UP | NA | NA | OFF | NA | NA | NA | 3.3
32/2 | dacrclk | out | IOB15[B] | - | LVCMOS33 | 8 | UP | NA | NA | OFF | NA | NA | NA | 3.3
33/2 | cpuclk | in | IOB23[A] | - | LVCMOS33 | NA | UP | ON | NONE | NA | NA | NA | NA | 3.3
34/2 | ncs | in | IOB23[B] | - | LVCMOS33 | NA | UP | ON | NONE | NA | NA | NA | NA | 3.3
35/2 | ps2data | io | IOB29[A] | GCLKT_4 | LVCMOS33 | 8 | NONE | NA | NONE | OFF | NA | NA | NA | 3.3
36/2 | disk_sck | out | IOB29[B] | GCLKC_4 | LVCMOS33 | 8 | UP | NA | NA | OFF | NA | NA | NA | 3.3
37/2 | disk_mosi | out | IOB31[A] | - | LVCMOS33 | 8 | UP | NA | NA | OFF | NA | NA | NA | 3.3
38/2 | - | in | IOB31[B] | - | LVCMOS33 | NA | UP | ON | NONE | NA | NA | NA | NA | 3.3
39/2 | disk_miso | in | IOB33[A] | - | LVCMOS33 | NA | UP | ON | NONE | NA | NA | NA | NA | 3.3
40/2 | intr_out | out | IOB33[B] | - | LVCMOS33 | 8 | NONE | NA | NA | OFF | NA | NA | NA | 3.3
41/2 | data[0] | io | IOB41[A] | - | LVCMOS33 | 8 | UP | NA | NONE | OFF | NA | NA | NA | 3.3
42/2 | data[1] | io | IOB41[B] | - | LVCMOS33 | 8 | UP | NA | NONE | OFF | NA | NA | NA | 3.3
47/2 | - | in | IOB43[B] | - | LVCMOS33 | NA | UP | ON | NONE | NA | NA | NA | NA | 3.3
p1-14/3 | - | in | IOL2[A] | - | LVCMOS18 | - | UP | - | - | - | - | - | - | -
p1-13/3 | - | in | IOL2[B] | - | LVCMOS18 | - | UP | - | - | - | - | - | - | -
p1-12/3 | - | in | IOL3[A] | - | LVCMOS18 | - | UP | - | - | - | - | - | - | -
p1-11/3 | - | in | IOL3[B] | - | LVCMOS18 | - | UP | - | - | - | - | - | - | -
p1-10/3 | - | in | IOL4[A] | - | LVCMOS18 | - | UP | - | - | - | - | - | - | -
4/3 | resetn | in | IOL5[A] | JTAGSEL_N/LPLL_T_in | LVCMOS18 | NA | UP | ON | NONE | NA | NA | OFF | NA | 1.8
p1-9/3 | - | in | IOL6[B] | LPLL_C_fb | LVCMOS18 | - | UP | - | - | - | - | - | - | -
p1-8/3 | - | in | IOL7[A] | - | LVCMOS18 | - | UP | - | - | - | - | - | - | -
p1-7/3 | - | in | IOL8[A] | - | LVCMOS18 | - | UP | - | - | - | - | - | - | -
p1-6/3 | - | in | IOL9[A] | GCLKT_7 | LVCMOS18 | - | UP | - | - | - | - | - | - | -
5/3 | - | in | IOL11[A] | TMS | LVCMOS18 | NA | UP | ON | NONE | NA | NA | NA | NA | 1.8
6/3 | - | in | IOL11[B] | TCK | LVCMOS18 | NA | UP | ON | NONE | NA | NA | NA | NA | 1.8
7/3 | - | in | IOL12[B] | TDI | LVCMOS18 | NA | UP | ON | NONE | NA | NA | NA | NA | 1.8
8/3 | - | out | IOL13[A] | TDO | LVCMOS18 | 8 | UP | NA | NA | OFF | NA | NA | NA | 1.8
9/3 | - | in | IOL13[B] | RECONFIG_N | LVCMOS18 | NA | UP | ON | NONE | NA | NA | NA | NA | 1.8
p1-5/3 | - | in | IOL14[A] | DONE | LVCMOS18 | - | UP | - | - | - | - | - | - | -
10/3 | led[0] | out | IOL15[A] | GCLKT_6 | LVCMOS18 | 8 | UP | NA | NA | OFF | NA | OFF | NA | 1.8
p1-4/3 | - | in | IOL16[A] | - | LVCMOS18 | - | UP | - | - | - | - | - | - | -
11/3 | led[1] | out | IOL16[B] | - | LVCMOS18 | 8 | UP | NA | NA | OFF | NA | OFF | NA | 1.8
p1-2/3 | - | in | IOL17[A] | - | LVCMOS18 | - | UP | - | - | - | - | - | - | -
p1-3/3 | - | in | IOL17[B] | - | LVCMOS18 | - | UP | - | - | - | - | - | - | -
p2-14/3 | - | in | IOL18[A] | - | LVCMOS18 | - | UP | - | - | - | - | - | - | -
p2-13/3 | - | in | IOL18[B] | - | LVCMOS18 | - | UP | - | - | - | - | - | - | -
p2-12/3 | - | in | IOL20[A] | - | LVCMOS18 | - | UP | - | - | - | - | - | - | -
p2-11/3 | - | in | IOL20[B] | - | LVCMOS18 | - | UP | - | - | - | - | - | - | -
p2-10/3 | - | in | IOL21[A] | - | LVCMOS18 | - | UP | - | - | - | - | - | - | -
13/3 | led[2] | out | IOL21[B] | - | LVCMOS18 | 8 | UP | NA | NA | OFF | NA | OFF | NA | 1.8
p2-9/3 | - | in | IOL22[A] | - | LVCMOS18 | - | UP | - | - | - | - | - | - | -
14/3 | led[3] | out | IOL22[B] | - | LVCMOS18 | 8 | UP | NA | NA | OFF | NA | OFF | NA | 1.8
p2-8/3 | - | in | IOL23[A] | - | LVCMOS18 | - | UP | - | - | - | - | - | - | -
p2-7/3 | - | in | IOL23[B] | - | LVCMOS18 | - | UP | - | - | - | - | - | - | -
p2-6/3 | - | in | IOL24[B] | - | LVCMOS18 | - | UP | - | - | - | - | - | - | -
p2-5/3 | - | in | IOL25[A] | - | LVCMOS18 | - | UP | - | - | - | - | - | - | -
15/3 | led[4] | out | IOL25[B] | - | LVCMOS18 | 8 | UP | NA | NA | OFF | NA | OFF | NA | 1.8
p2-4/3 | - | in | IOL26[A] | - | LVCMOS18 | - | UP | - | - | - | - | - | - | -
16/3 | led[5] | out | IOL26[B] | - | LVCMOS18 | 8 | UP | NA | NA | OFF | NA | OFF | NA | 1.8
p2-3/3 | - | in | IOL27[A] | - | LVCMOS18 | - | UP | - | - | - | - | - | - | -
p2-2/3 | - | in | IOL27[B] | - | LVCMOS18 | - | UP | - | - | - | - | - | - | -
63/1 | rts_serial | out | IOR5[A] | RPLL_T_in | LVCMOS33 | 8 | UP | NA | NA | OFF | NA | OFF | NA | 3.3
62/1 | - | in | IOR11[A] | MI/D7 | LVCMOS33 | NA | UP | ON | NONE | NA | NA | NA | NA | 3.3
61/1 | - | in | IOR11[B] | MO/D6 | LVCMOS33 | NA | UP | ON | NONE | NA | NA | NA | NA | 3.3
60/1 | - | in | IOR12[A] | MCS_N/D5 | LVCMOS33 | NA | UP | ON | NONE | NA | NA | NA | NA | 3.3
59/1 | - | in | IOR12[B] | MCLK/D4 | LVCMOS33 | NA | UP | ON | NONE | NA | NA | NA | NA | 3.3
57/1 | data[7] | io | IOR13[A] | FASTRD_N/D3 | LVCMOS33 | 8 | UP | NA | NONE | OFF | NA | OFF | NA | 3.3
56/1 | data[6] | io | IOR14[A] | SO/D1 | LVCMOS33 | 8 | UP | NA | NONE | OFF | NA | OFF | NA | 3.3
55/1 | data[5] | io | IOR14[B] | SSPI_CS_N/D0 | LVCMOS33 | 8 | UP | NA | NONE | OFF | NA | OFF | NA | 3.3
54/1 | data[4] | io | IOR15[A] | DIN/CLKHOLD_N | LVCMOS33 | 8 | UP | NA | NONE | OFF | NA | OFF | NA | 3.3
53/1 | data[3] | io | IOR15[B] | DOUT/WE_N | LVCMOS33 | 8 | UP | NA | NONE | OFF | NA | OFF | NA | 3.3
52/1 | clk | in | IOR17[A] | GCLKT_3 | LVCMOS33 | NA | UP | ON | NONE | NA | NA | OFF | NA | 3.3
51/1 | data[2] | io | IOR17[B] | GCLKC_3 | LVCMOS33 | 8 | UP | NA | NONE | OFF | NA | OFF | NA | 3.3
50/1 | - | in | IOR22[B] | - | LVCMOS33 | NA | UP | ON | NONE | NA | NA | NA | NA | 3.3
49/1 | dacser | out | IOR24[A] | - | LVCMOS33 | 8 | UP | NA | NA | OFF | NA | OFF | NA | 3.3
48/1 | - | in | IOR24[B] | - | LVCMOS33 | NA | UP | ON | NONE | NA | NA | NA | NA | 3.3